{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["review-comments"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"review-comments","index":0,"n_rows":2,"n_cols":10,"rows_kept":2,"cut":false,"hidden":false,"merged":[]}
["Comment ID","Commenting on behalf of","Organization","Comment","Supporting links","Supporting documents","Comment approved","Comment moderation","created","Link to comment"]
[46589,"in my professional capacity, on behalf of my organization","City of Barrie","The Corporation of the City of Barrie's Environmental Compliance Unit (City) has reviewed the ERO proposal and has the following comments to be taken into consideration when creating the maintenance and monitoring requirements of the proposed ECA: \n1. All stormwater entering the Municipal Storm Sewer System must comply with the City's Sewer Use By-law 2012-172 {By-law), as amended. \n2. Section 9.3 of the By-law outlines the requirements for Owners or Operators of a property that have an oil grit separator (OGS) installed. This includes:\n         a. ensuring the drainage from an OGS unit does not exceed the limits of the By-law,\n         b. OGS units are to be inspected and maintained as per manufacturers recommendations to ensure appropriate water quality control\n         c. all records pertaining to the maintenance and inspection of the OGS must be retained for a minimum of two (2) years\n3. The City recommends that the Owner be required to prepare an Operations Manual for the Stormwater Works that includes the following information\n        a. operating procedures for routine operation of the Works\n       b. inspection programs, including frequency of inspection, for the works and the methods or testes employed to detect when maintenance is necessary\n      c. repair and maintenance programs, including the frequency of repair and maintenance for the Works\n      d. procedures for the inspection and calibration of monitoring equipment\n      e. a spill prevention control and countermeasures plan, consisting of contingency plans and procedures for dealing with potential spills and any other abnormal situations",null,null,"Yes",null,"2020-06-17T15:19:00","comment/46589"]